


Task 1:

Step 1:






Task 2:



Task 2???




Debugging: (show content of registers, etc.)

Setup breakpoint

Many ways, in asm, the easiest way is to make a breakpoint in the first label.

Label such as \_start, \_exit, etc. They can be wtv u want



Print /x $ax

Disassemble

Ni

Set disassembly intel

